Output of 'file' command:
=========================
./build/arm-v6-hf/libftd2xx.so.1.3.6: ELF 32-bit LSB  shared object, ARM, EABI5 version 1 (SYSV), dynamically linked, BuildID[sha1]=7dd66d43c2207e82a8ef5c2178fb8ced870573dd, not stripped
Output of 'readelf -A' command:
===============================
Attribute Section: aeabi
File Attributes
  Tag_CPU_name: "6"
  Tag_CPU_arch: v6
  Tag_ARM_ISA_use: Yes
  Tag_THUMB_ISA_use: Thumb-1
  Tag_FP_arch: VFPv2
  Tag_ABI_PCS_wchar_t: 4
  Tag_ABI_FP_denormal: Needed
  Tag_ABI_FP_exceptions: Needed
  Tag_ABI_FP_number_model: IEEE 754
  Tag_ABI_align_needed: 8-byte
  Tag_ABI_align_preserved: 8-byte, except leaf SP
  Tag_ABI_enum_size: int
  Tag_ABI_HardFP_use: SP and DP
  Tag_ABI_VFP_args: VFP registers
  Tag_ABI_optimization_goals: Aggressive Speed
  Tag_CPU_unaligned_access: v6
  Tag_DIV_use: Not allowed
